	POSITION PROFILE
Equipment Operator
Northgate Contracting Ltd  ·  3 tasks  ·  3 competency checks  ·  3 with must-pass lines ◆



 1   Training required     Held before the work starts
	WHEN
	TRAINING
	WHY

	Before work
	Company safety orientation
	Every position

	Before work
	WHMIS 2025
	Every position

	Before work
	Hazard Assessment Training
	Every position

	Before work
	Harassment and Violence
	Every position

	Before the task
	Fall Protection Training
	Ladder Use

	Before the task
	Ground Disturbance 201
	Trenching and Excavating

	Before the task
	Overhead Electrical Utilities & Lines
	Skid Steer Use

	Before the task
	Skid Steer
	Skid Steer Use


 2   Competencies checked on the job     Competency record, signed Competent
	◆ Ladder Use
	HIGH
	◆ Trenching and Excavating
	HIGH

	◆ Skid Steer Use
	HIGH
	
	


◆ the record has must-pass lines.  Checked by a supervisor or a worker already signed Competent. Reassess every 3 years, or after a change to the task, new equipment or an incident.
 3   PPE for this position's tasks
Safety footwear  ·  Gloves  ·  Hard hat  ·  High-visibility clothing  ·  The designated signal person wears a high-visibility vest  ·  Seat belt  ·  Dust mask or respirator  ·  Hearing protection  ·  Safety glasses  ·  Designated signal person vest  ·  Full body harness  ·  Personal gas monitor
 4   Top hazards
Falls  ·  Falls from height  ·  Struck by traffic or other equipment during the walk-around  ·  Striking people or equipment nearby while testing controls  ·  Striking people, equipment or structures in a congested area  ·  Striking a buried utility because locate markers are missing
 5   Until signed Competent
A new or re-assigned worker in this position does a checked task only with a supervisor, or a worker signed Competent on that task, beside them.
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	POSITION PROFILE
Labourer
Northgate Contracting Ltd  ·  4 tasks  ·  4 competency checks  ·  2 with must-pass lines ◆



 1   Training required     Held before the work starts
	WHEN
	TRAINING
	WHY

	Before work
	Company safety orientation
	Every position

	Before work
	WHMIS 2025
	Every position

	Before work
	Hazard Assessment Training
	Every position

	Before work
	Harassment and Violence
	Every position

	Before the task
	Fall Protection Training
	Ladder Use

	Before the task
	Ground Disturbance 201
	Trenching and Excavating


 2   Competencies checked on the job     Competency record, signed Competent
	◆ Ladder Use
	HIGH
	Hand Tools Use
	MEDIUM

	◆ Trenching and Excavating
	HIGH
	Use of Power Tools
	MEDIUM


◆ the record has must-pass lines.  Checked by a supervisor or a worker already signed Competent. Reassess every 3 years, or after a change to the task, new equipment or an incident.
 3   PPE for this position's tasks
Safety footwear  ·  Gloves  ·  Hard hat  ·  Hearing protection  ·  Safety glasses  ·  High-visibility clothing  ·  Designated signal person vest  ·  Full body harness  ·  Personal gas monitor  ·  Dust mask or respirator  ·  Fire-resistant clothing
 4   Top hazards
Falls  ·  Falls from height  ·  Striking a buried utility because locate markers are missing  ·  Collapse of the hydrovac or hand-dug hole  ·  Operator unable to see workers or obstacles
 5   Until signed Competent
A new or re-assigned worker in this position does a checked task only with a supervisor, or a worker signed Competent on that task, beside them.
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